Voltage ok
Temperature ok
SYS FAN: Sensor SYS_FAN_A3_Fan1 critical low: current speed is 82 RPM, critical low is 1200 RPM
PSU 1 ok
PSU 2 ok
NVRAM7-temperature-0 ok
NVRAM7-battery-0 OK
--------------------------------------------------------------
Channel: 0a Shelf: 1 Shelf Serial Number: OPS677342115F62
Shelf product id: DS14-Mk4-FC
Module A Serial Number: IMS69813318D1BB  Firmware rev: 14
Module B Serial Number: IMS69813318D2AB  Firmware rev: 14
Controller A boot time: 1 days 5 hrs 21 mins 22 secs
Controller B boot time: 1 days 5 hrs 25 mins 53 secs
Power control state: ok
Last power control completion status: ok
Timestamp: Sun Aug 19 19:04:34 GMT 2018
--------------------------------------------------------------

Loop                   Drive            Drive     Command     5V     12V        Drive     Reset        Over     CtlLine
 ID                  Present            Power     Request                     Powered     Fault     Current       Stuck
                                       Status      Status                        Down                 Fault        OFF
0a.16                     X                Ok           -     ON      ON           -         -           -           -
0a.17                     X                Ok           -     ON      ON           -         -           -           -
0a.18                     X                Ok           -     ON      ON           -         -           -           -
0a.19                     X                Ok           -     ON      ON           -         -           -           -
0a.20                     X                Ok           -     ON      ON           -         -           -           -
0a.21                     X                Ok           -     ON      ON           -         -           -           -
0a.22                     X                Ok           -     ON      ON           -         -           -           -
0a.23                     X                Ok           -     ON      ON           -         -           -           -
0a.24                     X                Ok           -     ON      ON           -         -           -           -
0a.25                     X                Ok           -     ON      ON           -         -           -           -
0a.26                     X                Ok           -     ON      ON           -         -           -           -
0a.27                     X                Ok           -     ON      ON           -         -           -           -
0a.28                     X                Ok           -     ON      ON           -         -           -           -
0a.29                     X                Ok           -     ON      ON           -         -           -           -
--------------------------------------------------------------
Channel: 0a Shelf: 2 Shelf Serial Number: OPS6773421D3471
Shelf product id: DS14-Mk4-FC
Module A Serial Number: IMS69813319E247  Firmware rev: 14
Module B Serial Number: IMS69813319E2CB  Firmware rev: 14
Controller A boot time: 0 days 22 hrs 12 mins 26 secs
Controller B boot time: 0 days 22 hrs 14 mins 41 secs
Power control state: ok
Last power control completion status: ok
Timestamp: Sun Aug 19 19:04:34 GMT 2018
--------------------------------------------------------------

Loop                   Drive            Drive     Command     5V     12V        Drive     Reset        Over     CtlLine
 ID                  Present            Power     Request                     Powered     Fault     Current       Stuck
                                       Status      Status                        Down                 Fault        OFF
0a.32                     X                Ok           -     ON      ON           -         -           -           -
0a.33                     X                Ok           -     ON      ON           -         -           -           -
0a.34                     X                Ok           -     ON      ON           -         -           -           -
0a.35                     X                Ok           -     ON      ON           -         -           -           -
0a.36                     X                Ok           -     ON      ON           -         -           -           -
0a.37                     X                Ok           -     ON      ON           -         -           -           -
0a.38                     X                Ok           -     ON      ON           -         -           -           -
0a.39                     X                Ok           -     ON      ON           -         -           -           -
0a.40                     X                Ok           -     ON      ON           -         -           -           -
0a.41                     X                Ok           -     ON      ON           -         -           -           -
0a.42                     X                Ok           -     ON      ON           -         -           -           -
0a.43                     X                Ok           -     ON      ON           -         -           -           -
0a.44                     X                Ok           -     ON      ON           -         -           -           -
0a.45                     X                Ok           -     ON      ON           -         -           -           -
--------------------------------------------------------------
Channel: 0a Shelf: 3 Shelf Serial Number: OPS677342107C80
Shelf product id: DS14-Mk4-FC
Module A Serial Number: IMS698133127C99  Firmware rev: 14
Module B Serial Number: IMS698133127E4D  Firmware rev: 14
Controller A boot time: 1 days 5 hrs 22 mins 12 secs
Controller B boot time: 1 days 5 hrs 21 mins 17 secs
Power control state: ok
Last power control completion status: ok
Timestamp: Sun Aug 19 19:04:34 GMT 2018
--------------------------------------------------------------

Loop                   Drive            Drive     Command     5V     12V        Drive     Reset        Over     CtlLine
 ID                  Present            Power     Request                     Powered     Fault     Current       Stuck
                                       Status      Status                        Down                 Fault        OFF
0a.48                     X                Ok           -     ON      ON           -         -           -           -
0a.49                     X                Ok           -     ON      ON           -         -           -           -
0a.50                     X                Ok           -     ON      ON           -         -           -           -
0a.51                     X                Ok           -     ON      ON           -         -           -           -
0a.52                     X                Ok           -     ON      ON           -         -           -           -
0a.53                     X                Ok           -     ON      ON           -         -           -           -
0a.54                     X                Ok           -     ON      ON           -         -           -           -
0a.55                     X                Ok           -     ON      ON           -         -           -           -
0a.56                     X                Ok           -     ON      ON           -         -           -           -
0a.57                     X                Ok           -     ON      ON           -         -           -           -
0a.58                     X                Ok           -     ON      ON           -         -           -           -
0a.59                     X                Ok           -     ON      ON           -         -           -           -
0a.60                     X                Ok           -     ON      ON           -         -           -           -
0a.61                     X                Ok           -     ON      ON           -         -           -           -
--------------------------------------------------------------
Channel: 0c Shelf: 1 Shelf Serial Number: OPS67734211415B
Shelf product id: DS14-Mk4-FC
Module A Serial Number: IMS6981331901FD  Firmware rev: 14
Module B Serial Number: IMS698133185DCA  Firmware rev: 14
Controller A boot time: 0 days 22 hrs 7 mins 24 secs
Controller B boot time: 0 days 22 hrs 11 mins 10 secs
Power control state: ok
Last power control completion status: ok
Timestamp: Sun Aug 19 19:04:34 GMT 2018
--------------------------------------------------------------

Loop                   Drive            Drive     Command     5V     12V        Drive     Reset        Over     CtlLine
 ID                  Present            Power     Request                     Powered     Fault     Current       Stuck
                                       Status      Status                        Down                 Fault        OFF
0c.16                     X                Ok           -     ON      ON           -         -           -           -
0c.17                     X                Ok           -     ON      ON           -         -           -           -
0c.18                     X                Ok           -     ON      ON           -         -           -           -
0c.19                     X                Ok           -     ON      ON           -         -           -           -
0c.20                     X                Ok           -     ON      ON           -         -           -           -
0c.21                     X                Ok           -     ON      ON           -         -           -           -
0c.22                     X                Ok           -     ON      ON           -         -           -           -
0c.23                     X                Ok           -     ON      ON           -         -           -           -
0c.24                     X                Ok           -     ON      ON           -         -           -           -
0c.25                     X                Ok           -     ON      ON           -         -           -           -
0c.26                     X                Ok           -     ON      ON           -         -           -           -
0c.27                     X                Ok           -     ON      ON           -         -           -           -
0c.28                     X                Ok           -     ON      ON           -         -           -           -
0c.29                     X                Ok           -     ON      ON           -         -           -           -
--------------------------------------------------------------
Channel: 0c Shelf: 2 Shelf Serial Number: OPS677342200347
Shelf product id: DS14-Mk4-FC
Module A Serial Number: IMS69813312A430  Firmware rev: 14
Module B Serial Number: IMS6981331D9A1B  Firmware rev: 14
Controller A boot time: 1 days 6 hrs 14 mins 33 secs
Controller B boot time: 1 days 6 hrs 15 mins 26 secs
Power control state: ok
Last power control completion status: ok
Timestamp: Sun Aug 19 19:04:34 GMT 2018
--------------------------------------------------------------

Loop                   Drive            Drive     Command     5V     12V        Drive     Reset        Over     CtlLine
 ID                  Present            Power     Request                     Powered     Fault     Current       Stuck
                                       Status      Status                        Down                 Fault        OFF
0c.32                     X                Ok           -     ON      ON           -         -           -           -
0c.33                     X                Ok           -     ON      ON           -         -           -           -
0c.34                     X                Ok           -     ON      ON           -         -           -           -
0c.35                     X                Ok           -     ON      ON           -         -           -           -
0c.36                     X                Ok           -     ON      ON           -         -           -           -
0c.37                     X                Ok           -     ON      ON           -         -           -           -
0c.38                     X                Ok           -     ON      ON           -         -           -           -
0c.39                     X                Ok           -     ON      ON           -         -           -           -
0c.40                     X                Ok           -     ON      ON           -         -           -           -
0c.41                     X                Ok           -     ON      ON           -         -           -           -
0c.42                     X                Ok           -     ON      ON           -         -           -           -
0c.43                     X                Ok           -     ON      ON           -         -           -           -
0c.44                     X                Ok           -     ON      ON           -         -           -           -
0c.45                     X                Ok           -     ON      ON           -         -           -           -
--------------------------------------------------------------
Channel: 0c Shelf: 3 Shelf Serial Number: OPS67734210690C
Shelf product id: DS14-Mk4-FC
Module A Serial Number: IMS69813312E264  Firmware rev: 14
Module B Serial Number: IMS69813312E258  Firmware rev: 14
Controller A boot time: 1 days 6 hrs 40 mins 2 secs
Controller B boot time: 1 days 6 hrs 38 mins 3 secs
Power control state: ok
Last power control completion status: ok
Timestamp: Sun Aug 19 19:04:34 GMT 2018
--------------------------------------------------------------

Loop                   Drive            Drive     Command     5V     12V        Drive     Reset        Over     CtlLine
 ID                  Present            Power     Request                     Powered     Fault     Current       Stuck
                                       Status      Status                        Down                 Fault        OFF
0c.48                     X                Ok           -     ON      ON           -         -           -           -
0c.49                     X                Ok           -     ON      ON           -         -           -           -
0c.50                     X                Ok           -     ON      ON           -         -           -           -
0c.51                     X                Ok           -     ON      ON           -         -           -           -
0c.52                     X                Ok           -     ON      ON           -         -           -           -
0c.53                     X                Ok           -     ON      ON           -         -           -           -
0c.54                     X                Ok           -     ON      ON           -         -           -           -
0c.55                     X                Ok           -     ON      ON           -         -           -           -
0c.56                     X                Ok           -     ON      ON           -         -           -           -
0c.57                     X                Ok           -     ON      ON           -         -           -           -
0c.58                     X                Ok           -     ON      ON           -         -           -           -
0c.59                     X                Ok           -     ON      ON           -         -           -           -
0c.60                     X                Ok           -     ON      ON           -         -           -           -
0c.61                     X                Ok           -     ON      ON           -         -           -           -
--------------------------------------------------------------
Channel: 0c Shelf: 4 Shelf Serial Number: OPS677342106F9A
Shelf product id: DS14-Mk4-FC
Module A Serial Number: IMS69813312CFB0  Firmware rev: 14
Module B Serial Number: IMS69813312CF9A  Firmware rev: 14
Controller A boot time: 1 days 6 hrs 38 mins 4 secs
Controller B boot time: 1 days 6 hrs 39 mins 44 secs
Power control state: ok
Last power control completion status: ok
Timestamp: Sun Aug 19 19:04:34 GMT 2018
--------------------------------------------------------------

Loop                   Drive            Drive     Command     5V     12V        Drive     Reset        Over     CtlLine
 ID                  Present            Power     Request                     Powered     Fault     Current       Stuck
                                       Status      Status                        Down                 Fault        OFF
0c.64                     X                Ok           -     ON      ON           -         -           -           -
0c.65                     X                Ok           -     ON      ON           -         -           -           -
0c.66                     X                Ok           -     ON      ON           -         -           -           -
0c.67                     X                Ok           -     ON      ON           -         -           -           -
0c.68                     X                Ok           -     ON      ON           -         -           -           -
0c.69                     X                Ok           -     ON      ON           -         -           -           -
0c.70                     X                Ok           -     ON      ON           -         -           -           -
0c.71                     X                Ok           -     ON      ON           -         -           -           -
0c.72                     X                Ok           -     ON      ON           -         -           -           -
0c.73                     X                Ok           -     ON      ON           -         -           -           -
0c.74                     X                Ok           -     ON      ON           -         -           -           -
0c.75                     X                Ok           -     ON      ON           -         -           -           -
0c.76                     X                Ok           -     ON      ON           -         -           -           -
0c.77                     X                Ok           -     ON      ON           -         -           -           -
--------------------------------------------------------------
Channel: 0c Shelf: 5 Shelf Serial Number: OPS6773421C38D0
Shelf product id: DS14-Mk4-FC
Module A Serial Number: IMS69813319157F  Firmware rev: 14
Module B Serial Number: IMS698133190E53  Firmware rev: 14
Controller A boot time: 1 days 6 hrs 39 mins 48 secs
Controller B boot time: 1 days 6 hrs 37 mins 19 secs
Power control state: ok
Last power control completion status: ok
Timestamp: Sun Aug 19 19:04:34 GMT 2018
--------------------------------------------------------------

Loop                   Drive            Drive     Command     5V     12V        Drive     Reset        Over     CtlLine
 ID                  Present            Power     Request                     Powered     Fault     Current       Stuck
                                       Status      Status                        Down                 Fault        OFF
0c.80                     X                Ok           -     ON      ON           -         -           -           -
0c.81                     X                Ok           -     ON      ON           -         -           -           -
0c.82                     X                Ok           -     ON      ON           -         -           -           -
0c.83                     X                Ok           -     ON      ON           -         -           -           -
0c.84                     X                Ok           -     ON      ON           -         -           -           -
0c.85                     X                Ok           -     ON      ON           -         -           -           -
0c.86                     X                Ok           -     ON      ON           -         -           -           -
0c.87                     X                Ok           -     ON      ON           -         -           -           -
0c.88                     X                Ok           -     ON      ON           -         -           -           -
0c.89                     X                Ok           -     ON      ON           -         -           -           -
0c.90                     X                Ok           -     ON      ON           -         -           -           -
0c.91                     X                Ok           -     ON      ON           -         -           -           -
0c.92                     X                Ok           -     ON      ON           -         -           -           -
0c.93                     X                Ok           -     ON      ON           -         -           -           -
	Environment for channel 0a
	Number of shelves monitored: 3	enabled: yes
	Environmental failure on shelves on this channel? no

	Channel: 0a
	Shelf: 1
	SES device path: local access: 0a.17
	Module type: ESH4; monitoring is active  
	Shelf status: normal condition
	SES Configuration, via loop id 16 in shelf 1:
	 logical identifier=0x50050cc002115f62
	 vendor identification=XYRATEX
	 product identification=DS14-Mk4-FC
	 product revision level=1414
	Vendor-specific information:
	 Product Serial Number: OPS677342115F62
	 Optional Settings: 0x00
	Status reads attempted: 93; failed: 0
	Control writes attempted: 0; failed: 0
	Shelf bays with disk devices installed:
	  13, 12, 11, 10, 9, 8, 7, 6, 5, 4, 3, 2, 1, 0
	  with error: none
	Power Supply installed element list: 1, 2; with error: none
	Power Supply information by element:
	  [1] Serial number: PMC643620475134  Part number: <N/A>
	      Type: 5c
	      Firmware version: <N/A>  Swaps: 0
	  [2] Serial number: PMC643620475135  Part number: <N/A>
	      Type: 5c
	      Firmware version: <N/A>  Swaps: 0
	Power control element status: ok
	Cooling Unit installed element list: 1, 2; with error: none
	Temperature Sensor installed element list: 1, 2, 3; with error: none
	Shelf temperatures by element:
	  [1] 26 C (78 F) (ambient)  Normal temperature range
	  [2] 40 C (104 F)  Normal temperature range
	  [3] 38 C (100 F)  Normal temperature range
	Temperature thresholds by element:
	  [1] High critical: 50 C (122 F); high warning: 40 C (104 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	  [2] High critical: 63 C (145 F); high warning: 53 C (127 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	  [3] High critical: 63 C (145 F); high warning: 53 C (127 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	ES Electronics installed element list: 1, 2; with error: none
	ES Electronics reporting element: 1
	ES Electronics information by element:
	  [1] Serial number: IMS69813318D1BB  Part number: <N/A>
	      CPLD version: <N/A>  Swaps: 0
	  [2] Serial number: IMS69813318D2AB  Part number: <N/A>
	      CPLD version: <N/A>  Swaps: 0
	Embedded Switching Hub installed element list: 1, 2; with error: none


	Channel: 0a
	Shelf: 2
	SES device path: local access: 0a.33
	Module type: ESH4; monitoring is active  
	Shelf status: normal condition
	SES Configuration, via loop id 32 in shelf 2:
	 logical identifier=0x50050cc0021d3471
	 vendor identification=XYRATEX
	 product identification=DS14-Mk4-FC
	 product revision level=1414
	Vendor-specific information:
	 Product Serial Number: OPS6773421D3471
	 Optional Settings: 0x00
	Status reads attempted: 93; failed: 0
	Control writes attempted: 0; failed: 0
	Shelf bays with disk devices installed:
	  13, 12, 11, 10, 9, 8, 7, 6, 5, 4, 3, 2, 1, 0
	  with error: none
	Power Supply installed element list: 1, 2; with error: none
	Power Supply information by element:
	  [1] Serial number: PMC643620610309  Part number: <N/A>
	      Type: 5c
	      Firmware version: <N/A>  Swaps: 0
	  [2] Serial number: PMC643620610305  Part number: <N/A>
	      Type: 5c
	      Firmware version: <N/A>  Swaps: 0
	Power control element status: ok
	Cooling Unit installed element list: 1, 2; with error: none
	Temperature Sensor installed element list: 1, 2, 3; with error: none
	Shelf temperatures by element:
	  [1] 28 C (82 F) (ambient)  Normal temperature range
	  [2] 37 C (98 F)  Normal temperature range
	  [3] 35 C (95 F)  Normal temperature range
	Temperature thresholds by element:
	  [1] High critical: 50 C (122 F); high warning: 40 C (104 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	  [2] High critical: 63 C (145 F); high warning: 53 C (127 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	  [3] High critical: 63 C (145 F); high warning: 53 C (127 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	ES Electronics installed element list: 1, 2; with error: none
	ES Electronics reporting element: 1
	ES Electronics information by element:
	  [1] Serial number: IMS69813319E247  Part number: <N/A>
	      CPLD version: <N/A>  Swaps: 0
	  [2] Serial number: IMS69813319E2CB  Part number: <N/A>
	      CPLD version: <N/A>  Swaps: 0
	Embedded Switching Hub installed element list: 1, 2; with error: none


	Channel: 0a
	Shelf: 3
	SES device path: local access: 0a.48
	Module type: ESH4; monitoring is active  
	Shelf status: normal condition
	SES Configuration, via loop id 48 in shelf 3:
	 logical identifier=0x50050cc002107c80
	 vendor identification=XYRATEX
	 product identification=DS14-Mk4-FC
	 product revision level=1414
	Vendor-specific information:
	 Product Serial Number: OPS677342107C80
	 Optional Settings: 0x00
	Status reads attempted: 91; failed: 0
	Control writes attempted: 0; failed: 0
	Shelf bays with disk devices installed:
	  13, 12, 11, 10, 9, 8, 7, 6, 5, 4, 3, 2, 1, 0
	  with error: none
	Power Supply installed element list: 1, 2; with error: none
	Power Supply information by element:
	  [1] Serial number: PMA656670274551  Part number: <N/A>
	      Type: 74
	      Firmware version: <N/A>  Swaps: 0
	  [2] Serial number: PMC643620192372  Part number: <N/A>
	      Type: 5c
	      Firmware version: <N/A>  Swaps: 0
	Power control element status: ok
	Cooling Unit installed element list: 1, 2; with error: none
	Temperature Sensor installed element list: 1, 2, 3; with error: none
	Shelf temperatures by element:
	  [1] 27 C (80 F) (ambient)  Normal temperature range
	  [2] 37 C (98 F)  Normal temperature range
	  [3] 39 C (102 F)  Normal temperature range
	Temperature thresholds by element:
	  [1] High critical: 50 C (122 F); high warning: 40 C (104 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	  [2] High critical: 63 C (145 F); high warning: 53 C (127 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	  [3] High critical: 63 C (145 F); high warning: 53 C (127 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	ES Electronics installed element list: 1, 2; with error: none
	ES Electronics reporting element: 1
	ES Electronics information by element:
	  [1] Serial number: IMS698133127C99  Part number: <N/A>
	      CPLD version: <N/A>  Swaps: 0
	  [2] Serial number: IMS698133127E4D  Part number: <N/A>
	      CPLD version: <N/A>  Swaps: 0
	Embedded Switching Hub installed element list: 1, 2; with error: none

	Shelf mapping (shelf-assigned addresses) for channel 0a:
	  Shelf   1:  29  28  27  26  25  24  23  22  21  20  19  18  17  16
	  Shelf   2:  45  44  43  42  41  40  39  38  37  36  35  34  33  32
	  Shelf   3:  61  60  59  58  57  56  55  54  53  52  51  50  49  48

	Environment for channel 0c
	Number of shelves monitored: 5	enabled: yes
	Environmental failure on shelves on this channel? no

	Channel: 0c
	Shelf: 1
	SES device path: local access: 0c.17
	Module type: ESH4; monitoring is active  
	Shelf status: normal condition
	SES Configuration, via loop id 16 in shelf 1:
	 logical identifier=0x50050cc00211415b
	 vendor identification=XYRATEX
	 product identification=DS14-Mk4-FC
	 product revision level=1414
	Vendor-specific information:
	 Product Serial Number: OPS67734211415B
	 Optional Settings: 0x00
	Status reads attempted: 93; failed: 0
	Control writes attempted: 0; failed: 0
	Shelf bays with disk devices installed:
	  13, 12, 11, 10, 9, 8, 7, 6, 5, 4, 3, 2, 1, 0
	  with error: none
	Power Supply installed element list: 1, 2; with error: none
	Power Supply information by element:
	  [1] Serial number: PMC643620609017  Part number: <N/A>
	      Type: 5c
	      Firmware version: <N/A>  Swaps: 0
	  [2] Serial number: PMA656670299275  Part number: <N/A>
	      Type: 74
	      Firmware version: <N/A>  Swaps: 0
	Power control element status: ok
	Cooling Unit installed element list: 1, 2; with error: none
	Temperature Sensor installed element list: 1, 2, 3; with error: none
	Shelf temperatures by element:
	  [1] 26 C (78 F) (ambient)  Normal temperature range
	  [2] 41 C (105 F)  Normal temperature range
	  [3] 42 C (107 F)  Normal temperature range
	Temperature thresholds by element:
	  [1] High critical: 50 C (122 F); high warning: 40 C (104 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	  [2] High critical: 63 C (145 F); high warning: 53 C (127 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	  [3] High critical: 63 C (145 F); high warning: 53 C (127 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	ES Electronics installed element list: 1, 2; with error: none
	ES Electronics reporting element: 1
	ES Electronics information by element:
	  [1] Serial number: IMS6981331901FD  Part number: <N/A>
	      CPLD version: <N/A>  Swaps: 0
	  [2] Serial number: IMS698133185DCA  Part number: <N/A>
	      CPLD version: <N/A>  Swaps: 0
	Embedded Switching Hub installed element list: 1, 2; with error: none


	Channel: 0c
	Shelf: 2
	SES device path: local access: 0c.33
	Module type: ESH4; monitoring is active  
	Shelf status: normal condition
	SES Configuration, via loop id 32 in shelf 2:
	 logical identifier=0x50050cc002200347
	 vendor identification=XYRATEX
	 product identification=DS14-Mk4-FC
	 product revision level=1414
	Vendor-specific information:
	 Product Serial Number: OPS677342200347
	 Optional Settings: 0x00
	Status reads attempted: 91; failed: 0
	Control writes attempted: 0; failed: 0
	Shelf bays with disk devices installed:
	  13, 12, 11, 10, 9, 8, 7, 6, 5, 4, 3, 2, 1, 0
	  with error: none
	Power Supply installed element list: 1, 2; with error: none
	Power Supply information by element:
	  [1] Serial number: PMA944430038179  Part number: <N/A>
	      Type: HE Power Reset Capable (86)
	      Firmware version: <N/A>  Swaps: 0
	  [2] Serial number: PMW944430080523  Part number: <N/A>
	      Type: HE Power Reset Capable (86)
	      Firmware version: <N/A>  Swaps: 0
	  Auto power reset enabled: no
	Power control element status: ok
	Cooling Unit installed element list: 1, 2; with error: none
	Temperature Sensor installed element list: 1, 2, 3; with error: none
	Shelf temperatures by element:
	  [1] 27 C (80 F) (ambient)  Normal temperature range
	  [2] 34 C (93 F)  Normal temperature range
	  [3] 34 C (93 F)  Normal temperature range
	Temperature thresholds by element:
	  [1] High critical: 50 C (122 F); high warning: 40 C (104 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	  [2] High critical: 63 C (145 F); high warning: 53 C (127 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	  [3] High critical: 63 C (145 F); high warning: 53 C (127 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	ES Electronics installed element list: 1, 2; with error: none
	ES Electronics reporting element: 1
	ES Electronics information by element:
	  [1] Serial number: IMS69813312A430  Part number: <N/A>
	      CPLD version: <N/A>  Swaps: 0
	  [2] Serial number: IMS6981331D9A1B  Part number: <N/A>
	      CPLD version: <N/A>  Swaps: 0
	Embedded Switching Hub installed element list: 1, 2; with error: none


	Channel: 0c
	Shelf: 3
	SES device path: local access: 0c.49
	Module type: ESH4; monitoring is active  
	Shelf status: normal condition
	SES Configuration, via loop id 48 in shelf 3:
	 logical identifier=0x50050cc00210690c
	 vendor identification=XYRATEX
	 product identification=DS14-Mk4-FC
	 product revision level=1414
	Vendor-specific information:
	 Product Serial Number: OPS67734210690C
	 Optional Settings: 0x00
	Status reads attempted: 93; failed: 0
	Control writes attempted: 0; failed: 0
	Shelf bays with disk devices installed:
	  13, 12, 11, 10, 9, 8, 7, 6, 5, 4, 3, 2, 1, 0
	  with error: none
	Power Supply installed element list: 1, 2; with error: none
	Power Supply information by element:
	  [1] Serial number: PMC643620274080  Part number: <N/A>
	      Type: 5c
	      Firmware version: <N/A>  Swaps: 0
	  [2] Serial number: PMC643620274081  Part number: <N/A>
	      Type: 5c
	      Firmware version: <N/A>  Swaps: 0
	Power control element status: ok
	Cooling Unit installed element list: 1, 2; with error: none
	Temperature Sensor installed element list: 1, 2, 3; with error: none
	Shelf temperatures by element:
	  [1] 27 C (80 F) (ambient)  Normal temperature range
	  [2] 35 C (95 F)  Normal temperature range
	  [3] 36 C (96 F)  Normal temperature range
	Temperature thresholds by element:
	  [1] High critical: 50 C (122 F); high warning: 40 C (104 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	  [2] High critical: 63 C (145 F); high warning: 53 C (127 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	  [3] High critical: 63 C (145 F); high warning: 53 C (127 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	ES Electronics installed element list: 1, 2; with error: none
	ES Electronics reporting element: 1
	ES Electronics information by element:
	  [1] Serial number: IMS69813312E264  Part number: <N/A>
	      CPLD version: <N/A>  Swaps: 0
	  [2] Serial number: IMS69813312E258  Part number: <N/A>
	      CPLD version: <N/A>  Swaps: 0
	Embedded Switching Hub installed element list: 1, 2; with error: none


	Channel: 0c
	Shelf: 4
	SES device path: local access: 0c.64
	Module type: ESH4; monitoring is active  
	Shelf status: normal condition
	SES Configuration, via loop id 64 in shelf 4:
	 logical identifier=0x50050cc002106f9a
	 vendor identification=XYRATEX
	 product identification=DS14-Mk4-FC
	 product revision level=1414
	Vendor-specific information:
	 Product Serial Number: OPS677342106F9A
	 Optional Settings: 0x00
	Status reads attempted: 93; failed: 0
	Control writes attempted: 0; failed: 0
	Shelf bays with disk devices installed:
	  13, 12, 11, 10, 9, 8, 7, 6, 5, 4, 3, 2, 1, 0
	  with error: none
	Power Supply installed element list: 1, 2; with error: none
	Power Supply information by element:
	  [1] Serial number: PMA656670274385  Part number: <N/A>
	      Type: 74
	      Firmware version: <N/A>  Swaps: 0
	  [2] Serial number: PMA656670274387  Part number: <N/A>
	      Type: 74
	      Firmware version: <N/A>  Swaps: 0
	Power control element status: ok
	Cooling Unit installed element list: 1, 2; with error: none
	Temperature Sensor installed element list: 1, 2, 3; with error: none
	Shelf temperatures by element:
	  [1] 27 C (80 F) (ambient)  Normal temperature range
	  [2] 37 C (98 F)  Normal temperature range
	  [3] 39 C (102 F)  Normal temperature range
	Temperature thresholds by element:
	  [1] High critical: 50 C (122 F); high warning: 40 C (104 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	  [2] High critical: 63 C (145 F); high warning: 53 C (127 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	  [3] High critical: 63 C (145 F); high warning: 53 C (127 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	ES Electronics installed element list: 1, 2; with error: none
	ES Electronics reporting element: 1
	ES Electronics information by element:
	  [1] Serial number: IMS69813312CFB0  Part number: <N/A>
	      CPLD version: <N/A>  Swaps: 0
	  [2] Serial number: IMS69813312CF9A  Part number: <N/A>
	      CPLD version: <N/A>  Swaps: 0
	Embedded Switching Hub installed element list: 1, 2; with error: none


	Channel: 0c
	Shelf: 5
	SES device path: local access: 0c.81
	Module type: ESH4; monitoring is active  
	Shelf status: normal condition
	SES Configuration, via loop id 80 in shelf 5:
	 logical identifier=0x50050cc0021c38d0
	 vendor identification=XYRATEX
	 product identification=DS14-Mk4-FC
	 product revision level=1414
	Vendor-specific information:
	 Product Serial Number: OPS6773421C38D0
	 Optional Settings: 0x00
	Status reads attempted: 93; failed: 0
	Control writes attempted: 0; failed: 0
	Shelf bays with disk devices installed:
	  13, 12, 11, 10, 9, 8, 7, 6, 5, 4, 3, 2, 1, 0
	  with error: none
	Power Supply installed element list: 1, 2; with error: none
	Power Supply information by element:
	  [1] Serial number: PMC643620489576  Part number: <N/A>
	      Type: 5c
	      Firmware version: <N/A>  Swaps: 0
	  [2] Serial number: PMC643620489578  Part number: <N/A>
	      Type: 5c
	      Firmware version: <N/A>  Swaps: 0
	Power control element status: ok
	Cooling Unit installed element list: 1, 2; with error: none
	Temperature Sensor installed element list: 1, 2, 3; with error: none
	Shelf temperatures by element:
	  [1] 26 C (78 F) (ambient)  Normal temperature range
	  [2] 42 C (107 F)  Normal temperature range
	  [3] 40 C (104 F)  Normal temperature range
	Temperature thresholds by element:
	  [1] High critical: 50 C (122 F); high warning: 40 C (104 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	  [2] High critical: 63 C (145 F); high warning: 53 C (127 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	  [3] High critical: 63 C (145 F); high warning: 53 C (127 F)
	      Low critical:  0 C (32 F); low warning:  10 C (50 F)
	ES Electronics installed element list: 1, 2; with error: none
	ES Electronics reporting element: 1
	ES Electronics information by element:
	  [1] Serial number: IMS69813319157F  Part number: <N/A>
	      CPLD version: <N/A>  Swaps: 0
	  [2] Serial number: IMS698133190E53  Part number: <N/A>
	      CPLD version: <N/A>  Swaps: 0
	Embedded Switching Hub installed element list: 1, 2; with error: none

	Shelf mapping (shelf-assigned addresses) for channel 0c:
	  Shelf   1:  29  28  27  26  25  24  23  22  21  20  19  18  17  16
	  Shelf   2:  45  44  43  42  41  40  39  38  37  36  35  34  33  32
	  Shelf   3:  61  60  59  58  57  56  55  54  53  52  51  50  49  48
	  Shelf   4:  77  76  75  74  73  72  71  70  69  68  67  66  65  64
	  Shelf   5:  93  92  91  90  89  88  87  86  85  84  83  82  81  80

